Laser Direct Drive Inertial Confinement Fusion Research on OMEGA

S. P. Regan a, V. N. Goncharov a, T. C. Sangster a, E. M. Campbell a, R. Betti a, K. Anderson a, J. W. Bates c, K. Bauer a, T. P. Bernat d, S. D. Bhandarkar b, T. R. Boehly a, M. J. Bonino a, A. Bose a, D. Cao a, T. Chapman b, G. W. Collins a, T. J. B. Collins a, R. S. Craxton a, J. A. Delettrez a, D. H. Edgell a, R. Epstein a, M. Farrell e, C. J. Forrest a, J. A. Frenje f, D. H. Froula a, M. Gatu Johnson f, C. Gibson e, V. Yu. Glebov a, A. Greenwood e, D. R. Harding a, M. Hohenberger b, S. X. Hu a, H. Huang e, J. Hund d, I. V. Igumenshchev a, D. W. Jacobs-Perkins a, R. T. Janezic a, M. Karasik c, J. H. Kelly a, T. J. Kessler a, J. P. Knauer a, T. Z. Kosc a, J. A. Marozas a, F. J. Marshall a, P. W. McKenty a, D. T. Michel a, P. Michel b, J. D. Moody b, J. F. Myatt a, A. Nikroo b, S. P. Obenschain c, J. Palastro a, J. Peebles a, R. D. Petrasso f, N. Petta a, P. B. Radha a, J. E. Ralph b, M. J. Rosenberg a, S. Sampat a, A. J. Schmitt c, M. J. Schmitt g, M. Schoff e, W. Seka a, R. Shah a, R. W. Short a, W. T. Shmayda a, M. J. Shoup III a, A. Shvydky a, A. A. Solodov a, C. Sorce a, C. Stoeckl a, W. Sweet e, C. Taylor a, R. Taylora, W. Theobald a, D. Turnbull a, J. Ulreich a, M. D. Wittman a, K. M. Woo a, and J. D. Zuegel a

aLaboratory for Laser Energetics, University of Rochester, 250 E. River Rd., Rochester, NY 14623-1299, USA

bLawrence Livermore National Laboratory, USA

cNaval Research Laboratory, USA

dSchafer a Belcan company, USA

eGeneral Atomics, USA

fPlasma Science and Fusion Center, Massachusetts Institute of Technology, USA

gLos Alamos National Laboratory, USA

\*Corresponding author: sreg@lle.rochester.edu

**Abstract:** The objective of the multi-year, systematic 100-Gbar Campaign on the 30-kJ, 351-nm, 60-beam OMEGA laser system is to demonstrate and understand the physics for hot-spot conditions and formation relevant for ignition at the MJ scale. Laser direct drive ignition requires a hot-spot pressure above 120 Gbar for an ion temperature of 4 keV and an implosion convergence ratio above 22. The physics goals and the laser and target requirements of the hydrodynamically-scaled DT cryogenic implosions on OMEGA are derived from laser direct drive ignition target designs for a 1.8 MJ laser system (e.g., the National Ignition Facility). The strategy to increase the hot-spot pressure from the current level of ~60 Gbar is to reduce the long and short wavelength perturbations, mitigate LPI’s, and increase laser-to-target energy coupling. In parallel, a predictive capability that maps the relationship between the 1-D simulations and the experimental results is being used to optimize target performance. This talk will summarize the 100-Gbar Campaign on OMEGA.

This material is based upon work supported by the Department Of Energy National Nuclear Security Administration under Award Number DE‑NA0001944, Lawrence Livermore National Laboratory under Contract DE-AC52-07NA27344, the University of Rochester, and the New York State Energy Research and Development Authority. The support of DOE does not constitute an endorsement by DOE of the views expressed in the article.